Xyyzz

Low Pt Anodes for Polymer Electrolyte Fuel Cells

Jack Left (1), Mike Middle (1,2), Peter Wright (2)

(1) Fuel Cells Forever, Inc.

123 Efficiency Street, CH-1543 Clean Town/Wonderland

(2) Faculty of Sciences and Technology

Sample Street 45, DE-80801 New Town/Otherland

Tel.: +41-56-987-1234

Fax: +41-56-987-1235

[jsample@fastmail.com](mailto:jsample@fastmail.com)

Abstract

This here is a sample text: The reduction of the Pt catalyst loading in Polymer Electrolyte Fuel Cells (PEFC) is a premise for a commercial introduction of fuel cell electric cars. In the state of the art, the Pt loading for the anode varies between 30 and 100 µgr/sqcm. In this work, low platinum loadings in the range of 2 to 25 µgr/sqcm were sputtered onto carbon cloth substrates that were used as PEFC anodes. Membrane electrode assemblies were prepared by hot pressing with Nafion 212 and commercial cathodes. We succeeded in reducing the Pt loading of PEFC down to 25 µgr/sqcm without significant loss of fuel cell performance compared to commercial electrodes 500 µgr/sqcm. Longevity tests at constant current densities showed nearby stable voltages for at least 1’000 hrs. ………

Xyyzz

**Instructions:**

1. **Abstract Page** must not be longer than **1 page** (a graphic or a picture is very welcome).
2. Xyyzz must be left **untouched**.
3. **Rename the File** as follows:  
    **Short-title\_Family-name\_Given-name\_Current-Version.docx**e.g. PEFC-MembraneConductivity\_LowPtAnodePEFC\_Jack-Left\_01.docx.  
   Number "\_01" is for first submitted version, "\_02" for the second, etc.
4. **Overwrite the Sample Text** with your content,but **keep the formats** as given in this template.   
   See also the "Extended Instruction for Abstract and Paper preparation".
5. **Author-Institution Numbering:**  
   Do not write "**(1)...**" in the header, if there is only **one** institution, i.e. use the template below.
6. **Delete** all unused **templates** andthe gray **comment box** with the **red text** here.
7. **Register as an Author** on [www.EFCF.com/AC](http://www.EFCF.com/AC) (Author Centre).
   * Upload your one-page Abstract by **15th February 2021** at the latest.  
     [www.EFCF.com/Upload](http://www.EFCF.com/Upload)
   * Indicate the relevant **Topics** for your contribution and your preference: **Oral** or **Poster**.
8. Receive notification about **acceptance in March 2021**. This requires you to submit an **extended abstract/paper by 31 May 2021**. This is a **condition:**

* to be included in the **final program**
* to be given the opportunity that the contribution is **published** with an own **DOI** in the EFCF community of the general-purpose open-access repository [www.Zenodo.org](http://www.Zenodo.org).
* to be evaluated for inclusion in the **Special Issue** of the peer reviewed **Journal:**“Fuel Cells – From Fundamentals to Systems“ from Wiley-VCH[www.fuelcells.wiley-vch.de](http://www.fuelcells.wiley-vch.de)

**S**ee the **Publication Policy** [www.EFCF.com/PP](http://www.EFCF.com/PP)

Low Pt Anodes for Polymer Electrolyte Fuel Cells

**Template**

with **only one institution**

no (1) etc. required

Jack Left, Mike Middle, Peter Wright

Fuel Cells Forever, Inc.

123 Efficiency Street, CH-1543 Clean Town/Wonderland

Tel.: +41-56-987-1234

Fax: +41-56-987-1235

[jsample@fastmail.com](mailto:jsample@fastmail.com)

Abstract

This here is a sample text: The reduction of the Pt catalyst loading in Polymer Electrolyte Fuel Cells (PEFC) is a premise for a commercial introduction of fuel cell electric cars. In the state of the art, the Pt loading for the anode varies between 30 and 100 µgr/sqcm. In this work, low platinum loadings in the range of 2 to 25 µgr/sqcm were sputtered onto carbon cloth substrates that were used as PEFC anodes. Membrane electrode assemblies were prepared by hot pressing with Nafion 212 and commercial cathodes. We succeeded in reducing the Pt loading of PEFC down to 25 µgr/sqcm without significant loss of fuel cell performance compared to commercial electrodes 500 µgr/sqcm. Longevity tests at constant current densities showed nearby stable voltages for at least 1’000 hrs. ………