Xyyzz

Combustion synthesis of LaNi0.6Fe0.4O3 perovskite  
as cathode contact material for IT-SOFCs

|  |
| --- |
| Jack Left (1), Mike Middle (1,2), Peter Wright (2) |
| (1) Fuel Cells Forever, Inc. |
| 123 Efficiency Street, CH-1543 Clean Town/Wonderland |
| (2) Faculty of Sciences and Technology |
| 45 Sample Street, CH-8016 New Town/Wonderland |
| Tel.: +41-56-987-1234 |
| [jsample@fastmail.com](mailto:jsample@fastmail.com) |

Abstract

This is a sample text: Perovskite sample of composition LaNi0.6Fe0.4O3 has been prepared by the glycinenitrate route using different amounts of glycine fuel (G/N= 0.5, 1.0 and 1.5), in order to study the sample preparation influence on the structural, morphological and electrical properties in the context of their possible use as cathode contact material for intermediate temperature solid oxide fuel cells (IT-SOFCs). The obtained materials have been characterized by X-ray diffraction (XRD), scanning electron microscopy (SEM), thermal expansion coefficient (TEC) and electrical conductivity measurements. X-ray powder diffraction (XRD) shows that all of the compounds have rhombohedral symmetry (space group: R-3c). All of the samples obtained using different amounts of glycine fuel have a porous microstructure with fine grain sizes.

**Instructions:**

* First of all: go to [www.EFCF.com/**Like2Present**](http://www.EFCF.com/Like2Present) &   
  announce the TITLE & the DATE by which you will upload.  
  We need this information urgently, because the evaluation has started and it will be more and more difficult to consider uploads for **oral presentation**.   
  **Poster** contributions can be accepted for longer, but please announce them also, otherwise they might not be listed in the announcements any more.
* **Abstract Page** must not be longer than **1 page** (a graphic or a picture is very welcome).
* Xyyzz must be left **untouched**.
* **Rename the File**: **Short-title\_Family-name\_Given-name\_Current-Version.docx**e.g. CombustionSyntCatMatSOFC\_Jack-Left\_01.docx.  
  (Number "\_**01**" is for first submitted version, "\_**02**" for the second, if necessary, etc.)
* **Overwrite the Sample Text** with your content,but **keep the formats** as given in this template. See also the "Extended Instruction for Abstract preparation".
* **Author-Institution Numbering:** Do not write "**(1)...**" in the header,   
   if there is only **one** institution.
* **Delete all unused templates and the red comments here**.
* **Register as an Author** at [www.EFCF.com/AC](http://www.EFCF.com/AC) (Author Centre).
* Upload your one-page Abstract as announced on [www.EFCF.com/Upload](http://www.EFCF.com/Upload)
* Indicate the most relevant **Topics** for your contribution & the preference: **Oral/Poster**.

**Publication Policy:** see [www.EFCF.com/PP](http://www.EFCF.com/PP)A limited number of contributions are invited for inclusion in a **Special Issue** of peer reviewed **journal Fuel Cells** [www.fuelcells.wiley-vch.de](http://www.fuelcells.wiley-vch.de/). All contributions, that **request it**, will be **published** in the **open-access repository Zenodo** with a **DOI -** see [www.EFCF.com/DOI](http://www.EFCF.com/DOI).

Xyyzz

Combustion synthesis of LaNi0.6Fe0.4O3 perovskite  
as cathode contact material for IT-SOFCs

**Template**

with **only one institution**

no (1) etc. required

|  |
| --- |
| Jack Left, Mike Middle, Peter Wright |
| Fuel Cells Forever, Inc. |
| 123 Efficiency Street, CH-1543 Clean Town/Wonderland |
| Tel.: +41-56-987-1234 |
| [jsample@fastmail.com](mailto:jsample@fastmail.com) |

Abstract

This is a sample text: Perovskite sample of composition LaNi0.6Fe0.4O3 has been prepared by the glycinenitrate route using different amounts of glycine fuel (G/N= 0.5, 1.0 and 1.5), in order to study the sample preparation influence on the structural, morphological and electrical properties in the context of their possible use as cathode contact material for intermediate temperature solid oxide fuel cells (IT-SOFCs). The obtained materials have been characterized by X-ray diffraction (XRD), scanning electron microscopy (SEM), thermal expansion coefficient (TEC) and electrical conductivity measurements. X-ray powder diffraction (XRD) shows that all of the compounds have rhombohedral symmetry (space group: R-3c). All of the samples obtained using different amounts of glycine fuel have a porous microstructure with fine grain sizes.