Xyyzz

Low Pt Anodes for Polymer Electrolyte Fuel Cells

Jack Left (1), Mike Middle (1,2), Peter Wright (2)

(1) Fuel Cells Forever, Inc., Clean Town/ New Wonderland;

(2) Faculty of Sciences and Technology, New Town/Wonderland;

Tel.: +41-56-987-1234, Mobile: +41-22-333-444

[jsample@fastmail.com](mailto:jsample@fastmail.com)

Abstract

This here is a sample text: The reduction of the Pt catalyst loading in Polymer Electrolyte Fuel Cells (PEFC) is a premise for a commercial introduction of fuel cell electric cars. In the state of the art, the Pt loading for the anode varies between 30 and 100 µgr/sqcm. In this work, low platinum loadings in the range of 2 to 25 µgr/sqcm were sputtered onto carbon cloth substrates that were used as PEFC anodes. Membrane electrode assemblies were prepared by hot pressing with Nafion 212 and commercial cathodes. We succeeded in reducing the Pt loading of PEFC down to 25 µgr/sqcm without significant loss of fuel cell performance compared to commercial electrodes 500 µgr/sqcm. Longevity tests at constant current densities showed nearby stable voltages for at least 1’000 hrs. ………

**Instructions:**

* **Abstract Page** must not be longer than **1 page** (a graphic or a picture is very welcome).
* Xyyzz must be left **untouched**.
* **Rename the File** as follows:  
  **Short-title\_Family-name\_Given-name\_Current-Version.docx**e.g. PEFC-MembraneConductivity\_LowPtAnodePEFC\_Jack-Left\_01.docx.  
  (Number "\_**01**" is for first submitted version, "\_**02**" for the second, etc.)
* **Overwrite the Sample Text** with your content,but **keep the formats** as given in this template. See also the "Extended Instruction for Abstract and Paper preparation".
* **Author-Institution Numbering:** Do not write "**(1)...**" in the header, if there  
   is only **one** institution, i.e. use the template below.
* **Delete all unused templates and the red comments here**.
* **Register as an Author** on [www.EFCF.com/AC](http://www.EFCF.com/AC) (Author Centre).
  + Upload your one-page Abstract by **30th November 2022** at the latest.  
    [www.EFCF.com/Upload](http://www.EFCF.com/Upload)
  + Indicate the most relevant **Topic** for your contribution.
  + Indicate your Preference: **Oral** or **Poster**.

**Publication Policy:** see [www.EFCF.com/PP](http://www.EFCF.com/PP)A limited number of contributions will be invited for inclusion in a **Special Issue of the peer reviewed journal Fuel Cells –** [www.fuelcells.wiley-vch.de](http://www.fuelcells.wiley-vch.de/).

Xyyzz

Low Pt Anodes for Polymer Electrolyte Fuel Cells

**Template**

with **only one institution**

no (1) etc. required

Jack Left, Mike Middle, Peter Wright

Fuel Cells Forever, Inc., Clean Town/Wonderland

Tel.: +41-56-987-1234, Mobile: +41-22-333-444

[jsample@fastmail.com](mailto:jsample@fastmail.com)

Abstract

This here is a sample text: The reduction of the Pt catalyst loading in Polymer Electrolyte Fuel Cells (PEFC) is a premise for a commercial introduction of fuel cell electric cars. In the state of the art, the Pt loading for the anode varies between 30 and 100 µgr/sqcm. In this work, low platinum loadings in the range of 2 to 25 µgr/sqcm were sputtered onto carbon cloth substrates that were used as PEFC anodes. Membrane electrode assemblies were prepared by hot pressing with Nafion 212 and commercial cathodes. We succeeded in reducing the Pt loading of PEFC down to 25 µgr/sqcm without significant loss of fuel cell performance compared to commercial electrodes 500 µgr/sqcm. Longevity tests at constant current densities showed nearby stable voltages for at least 1’000 hrs. ………